Regulator test conditions

Input – 5V, 1.5A wall socket power supply

Radio settings – Tx Power 15dBm

Default (2) settings – slow & long range

* BW – 31.25kHz
* Coding rate – 4/8
* Spreading factor – 9 = 512 chips/symbol
* CRC on